<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.2.2">
<drawing>
<board>
<plain>
<wire x1="1.275078125" y1="-0.002540625" x2="23.370740625" y2="-0.002540625" width="0" layer="20"/>
<wire x1="23.370740625" y1="-0.002540625" x2="23.368" y2="51.054" width="0" layer="20"/>
<wire x1="23.368" y1="51.054" x2="25.654" y2="52.829459375" width="0" layer="20"/>
<wire x1="25.654" y1="52.829459375" x2="25.6541" y2="52.86491875" width="0" layer="20"/>
<wire x1="25.6541" y1="52.86491875" x2="25.6541" y2="56.134" width="0" layer="20"/>
<wire x1="25.6541" y1="56.134" x2="-0.2541" y2="56.12891875" width="0" layer="20"/>
<wire x1="-0.2541" y1="56.12891875" x2="-0.2541" y2="52.8321" width="0" layer="20"/>
<wire x1="-0.2541" y1="52.8321" x2="1.026159375" y2="50.28438125" width="0" layer="20"/>
<wire x1="1.026159375" y1="50.28438125" x2="1.275078125" y2="-0.002540625" width="0" layer="20"/>
<text>1541 Parallel adapter v1.1
Copyright (c) 2018
http://retro-commodore.eu
Greets to Peter Schepers</text>
<text>1</text>
<text>Solder Side</text>
</plain>
<libraries>
<library name="ic-package">
<description>&lt;b&gt;IC Packages an Sockets&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="DIL40">
<description>&lt;b&gt;Dual In Line Package&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="adafruit">
<packages>
<package name="1X10-BIG">
</package>
</packages>
</library>
<library name="1541-parallel">
<description>Generated from &lt;b&gt;1541-parallel.sch&lt;/b&gt;&lt;p&gt;
by exp-lbrs.ulp</description>
<packages>
<package name="IC-PACKAGE_DIL40">
<description>&lt;b&gt;Dual In Line Package&lt;/b&gt;</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="IC1" library="1541-parallel" package="IC-PACKAGE_DIL40" value="">
<attribute name="VALUE"/>
</element>
<element name="IC2" library="ic-package" package="DIL40" value="MOS6526">
<attribute name="SPICEPREFIX" value="X"/>
<attribute name="VALUE"/>
</element>
<element name="U$1" library="adafruit" package="1X10-BIG" value="PINHD-1X10"/>
</elements>
<signals>
<signal name="N$1">
<contactref element="IC2" pad="1"/>
<contactref element="IC1" pad="1"/>
</signal>
<signal name="N$2">
<contactref element="IC2" pad="3"/>
<contactref element="IC1" pad="3"/>
<contactref element="U$1" pad="2"/>
</signal>
<signal name="N$3">
<contactref element="IC1" pad="4"/>
<contactref element="IC2" pad="4"/>
<contactref element="U$1" pad="3"/>
</signal>
<signal name="N$4">
<contactref element="IC1" pad="5"/>
<contactref element="IC2" pad="5"/>
<contactref element="U$1" pad="4"/>
</signal>
<signal name="N$5">
<contactref element="IC2" pad="6"/>
<contactref element="IC1" pad="6"/>
<contactref element="U$1" pad="5"/>
</signal>
<signal name="N$6">
<contactref element="IC1" pad="7"/>
<contactref element="IC2" pad="7"/>
<contactref element="U$1" pad="6"/>
</signal>
<signal name="N$7">
<contactref element="IC2" pad="8"/>
<contactref element="IC1" pad="8"/>
<contactref element="U$1" pad="7"/>
</signal>
<signal name="N$8">
<contactref element="IC1" pad="9"/>
<contactref element="IC2" pad="9"/>
<contactref element="U$1" pad="8"/>
</signal>
<signal name="N$9">
<contactref element="IC2" pad="10"/>
<contactref element="IC1" pad="10"/>
</signal>
<signal name="N$10">
<contactref element="IC1" pad="11"/>
<contactref element="IC2" pad="11"/>
</signal>
<signal name="N$11">
<contactref element="IC2" pad="12"/>
<contactref element="IC1" pad="12"/>
</signal>
<signal name="N$12">
<contactref element="IC1" pad="13"/>
<contactref element="IC2" pad="13"/>
</signal>
<signal name="N$13">
<contactref element="IC2" pad="14"/>
<contactref element="IC1" pad="14"/>
</signal>
<signal name="N$14">
<contactref element="IC1" pad="15"/>
<contactref element="IC2" pad="15"/>
</signal>
<signal name="N$15">
<contactref element="IC2" pad="16"/>
<contactref element="IC1" pad="16"/>
</signal>
<signal name="N$16">
<contactref element="IC1" pad="17"/>
<contactref element="IC2" pad="17"/>
</signal>
<signal name="N$17">
<contactref element="IC2" pad="18"/>
<contactref element="IC1" pad="18"/>
<contactref element="U$1" pad="9"/>
</signal>
<signal name="N$18">
<contactref element="IC1" pad="19"/>
<contactref element="IC2" pad="19"/>
</signal>
<signal name="N$19">
<contactref element="IC2" pad="20"/>
<contactref element="IC1" pad="20"/>
</signal>
<signal name="N$20">
<contactref element="IC1" pad="21"/>
<contactref element="IC2" pad="21"/>
</signal>
<signal name="N$21">
<contactref element="IC2" pad="22"/>
<contactref element="IC1" pad="22"/>
</signal>
<signal name="N$22">
<contactref element="IC1" pad="23"/>
<contactref element="IC2" pad="23"/>
</signal>
<signal name="N$23">
<contactref element="IC2" pad="24"/>
<contactref element="IC1" pad="24"/>
</signal>
<signal name="N$24">
<contactref element="IC1" pad="25"/>
<contactref element="IC2" pad="25"/>
</signal>
<signal name="N$25">
<contactref element="IC2" pad="26"/>
<contactref element="IC1" pad="26"/>
</signal>
<signal name="N$26">
<contactref element="IC1" pad="27"/>
<contactref element="IC2" pad="27"/>
</signal>
<signal name="N$27">
<contactref element="IC2" pad="28"/>
<contactref element="IC1" pad="28"/>
</signal>
<signal name="N$28">
<contactref element="IC1" pad="29"/>
<contactref element="IC2" pad="29"/>
</signal>
<signal name="N$29">
<contactref element="IC2" pad="30"/>
<contactref element="IC1" pad="30"/>
</signal>
<signal name="N$30">
<contactref element="IC1" pad="31"/>
<contactref element="IC2" pad="31"/>
</signal>
<signal name="N$31">
<contactref element="IC2" pad="32"/>
<contactref element="IC1" pad="32"/>
</signal>
<signal name="N$32">
<contactref element="IC1" pad="33"/>
<contactref element="IC2" pad="33"/>
</signal>
<signal name="N$33">
<contactref element="IC2" pad="34"/>
<contactref element="IC1" pad="34"/>
</signal>
<signal name="N$34">
<contactref element="IC1" pad="35"/>
<contactref element="IC2" pad="35"/>
</signal>
<signal name="N$35">
<contactref element="IC2" pad="36"/>
<contactref element="IC1" pad="36"/>
</signal>
<signal name="N$36">
<contactref element="IC1" pad="37"/>
<contactref element="IC2" pad="37"/>
</signal>
<signal name="N$37">
<contactref element="IC1" pad="38"/>
<contactref element="IC2" pad="38"/>
</signal>
<signal name="N$38">
<contactref element="IC2" pad="39"/>
<contactref element="IC1" pad="39"/>
<contactref element="U$1" pad="10"/>
</signal>
<signal name="N$39">
<contactref element="IC1" pad="40"/>
<contactref element="IC2" pad="40"/>
</signal>
<signal name="N$40">
<contactref element="IC2" pad="2"/>
<contactref element="U$1" pad="1"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
