<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.5.2">
<drawing>
<board>
<plain>
<wire x1="0.635" y1="9.2964" x2="0.635" y2="1.2357" width="0" layer="20"/>
<wire x1="0.635" y1="1.2357" x2="1.8707" y2="0" width="0" layer="20" curve="90"/>
<wire x1="1.8707" y1="0" x2="56.51850625" y2="0" width="0" layer="20"/>
<wire x1="56.51850625" y1="0" x2="57.7979" y2="1.27939375" width="0" layer="20" curve="90"/>
<wire x1="57.7979" y1="1.27939375" x2="57.7979" y2="9.2906875" width="0" layer="20"/>
<wire x1="57.7979" y1="9.2906875" x2="57.9054125" y2="9.398165625" width="0" layer="20" curve="-90.018325"/>
<wire x1="57.9054125" y1="9.398165625" x2="57.943953125" y2="9.398153125" width="0" layer="20"/>
<wire x1="57.943953125" y1="9.398153125" x2="58.42" y2="9.874046875" width="0" layer="20" curve="90.035748"/>
<wire x1="58.42" y1="9.874046875" x2="58.42" y2="70.58" width="0" layer="20"/>
<wire x1="58.42" y1="70.58" x2="60.2385375" y2="70.58" width="0" layer="20"/>
<wire x1="60.2385375" y1="70.58" x2="62.23" y2="72.5714625" width="0" layer="20" curve="90"/>
<wire x1="62.23" y1="72.5714625" x2="62.23" y2="79.73691875" width="0" layer="20"/>
<wire x1="62.23" y1="79.73691875" x2="59.95691875" y2="82.00988125" width="0" layer="20" curve="90.002993"/>
<wire x1="59.95691875" y1="82.00988125" x2="58.4202" y2="82.0098" width="0" layer="20"/>
<wire x1="58.4202" y1="82.0098" x2="58.4202" y2="83.24" width="0" layer="20"/>
<wire x1="58.4202" y1="83.24" x2="0" y2="83.24" width="0" layer="20"/>
<wire x1="0" y1="83.24" x2="0" y2="9.9314" width="0" layer="20"/>
<wire x1="0" y1="9.9314" x2="0.5334" y2="9.398" width="0" layer="20" curve="90"/>
<wire x1="0.5334" y1="9.398" x2="0.635" y2="9.2964" width="0" layer="20" curve="-90"/>
<text>RCEU2215 - Cartridge Horizontal Adapter v1.0.2
Copyright (c) 2018-2020 http://retro-commodore.eu</text>
</plain>
<libraries>
<library name="C64CartridgeEdgeConnector">
<description>C64 Cartridge/Expansion edge connector</description>
<packages>
<package name="0RB_COMMODORE_MA100-22-2">
</package>
</packages>
</library>
<library name="SparkFun-Switches">
<description>&lt;h3&gt;SparkFun Switches, Buttons, Encoders&lt;/h3&gt;
In this library you'll find switches, buttons, joysticks, and anything that moves to create or disrupt an electrical connection.
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="TACTILE_SWITCH_PTH_RIGHT_ANGLE_KIT">
<description>&lt;h3&gt;Momentary Switch (Pushbutton) - SPST - PTH, Right-angle&lt;/h3&gt;
&lt;p&gt;Normally-open (NO) SPST momentary switches (buttons, pushbuttons).&lt;/p&gt;
&lt;p&gt;&lt;a href="http://cdn.sparkfun.com/datasheets/Components/Switches/SW016.JPG"&gt;Dimensional Drawing&lt;/a&gt;&lt;/p&gt;</description>
</package>
</packages>
</library>
<library name="con-samtec">
<description>&lt;b&gt;Samtec Connectors&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="TSW-122-XX-G-Q">
<description>&lt;b&gt;THROUGH-HOLE .025" SQ POST HEADER&lt;/b&gt;&lt;p&gt;
Source: Samtec TSW.pdf</description>
</package>
</packages>
</library>
<library name="holes">
<description>&lt;b&gt;Mounting Holes and Pads&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="3,0">
<description>&lt;b&gt;MOUNTING HOLE&lt;/b&gt; 3.0 mm with drill center</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="IC1" library="C64CartridgeEdgeConnector" package="0RB_COMMODORE_MA100-22-2" value="0RB_COMMODORE_EXPANSION_PORT_C64"/>
<element name="S1" library="SparkFun-Switches" package="TACTILE_SWITCH_PTH_RIGHT_ANGLE_KIT" value="MOMENTARY-SWITCH-SPST-PTH-RIGHT-ANGLE-KIT">
<attribute name="PROD_ID" value="CONN-10672"/>
<attribute name="SF_SKU" value="COM-10791"/>
</element>
<element name="X4" library="con-samtec" package="TSW-122-XX-G-Q" value="TSW-122-07-G-Q">
<attribute name="MF" value="Samtec Inc."/>
<attribute name="MPN" value="TSW-122-07-G-Q"/>
<attribute name="VALUE"/>
</element>
<element name="U$1" library="holes" package="3,0" value=""/>
<element name="U$2" library="holes" package="3,0" value=""/>
</elements>
<signals>
<signal name="VCC">
<contactref element="IC1" pad="2"/>
<contactref element="IC1" pad="3"/>
<contactref element="X4" pad="4"/>
<contactref element="X4" pad="6"/>
</signal>
<signal name="GND">
<contactref element="IC1" pad="1"/>
<contactref element="IC1" pad="22"/>
<contactref element="IC1" pad="A"/>
<contactref element="IC1" pad="Z"/>
<contactref element="X4" pad="1"/>
<contactref element="X4" pad="43"/>
<contactref element="X4" pad="2"/>
<contactref element="X4" pad="44"/>
<contactref element="S1" pad="2"/>
</signal>
<signal name="D7">
<contactref element="IC1" pad="14"/>
<contactref element="X4" pad="28"/>
</signal>
<signal name="D6">
<contactref element="IC1" pad="15"/>
<contactref element="X4" pad="30"/>
</signal>
<signal name="D5">
<contactref element="IC1" pad="16"/>
<contactref element="X4" pad="32"/>
</signal>
<signal name="D4">
<contactref element="IC1" pad="17"/>
<contactref element="X4" pad="34"/>
</signal>
<signal name="D3">
<contactref element="IC1" pad="18"/>
<contactref element="X4" pad="36"/>
</signal>
<signal name="D2">
<contactref element="IC1" pad="19"/>
<contactref element="X4" pad="38"/>
</signal>
<signal name="D1">
<contactref element="IC1" pad="20"/>
<contactref element="X4" pad="40"/>
</signal>
<signal name="D0">
<contactref element="IC1" pad="21"/>
<contactref element="X4" pad="42"/>
</signal>
<signal name="A0">
<contactref element="IC1" pad="Y"/>
<contactref element="X4" pad="41"/>
</signal>
<signal name="A1">
<contactref element="IC1" pad="X"/>
<contactref element="X4" pad="39"/>
</signal>
<signal name="A2">
<contactref element="IC1" pad="W"/>
<contactref element="X4" pad="37"/>
</signal>
<signal name="A3">
<contactref element="IC1" pad="V"/>
<contactref element="X4" pad="35"/>
</signal>
<signal name="A4">
<contactref element="IC1" pad="U"/>
<contactref element="X4" pad="33"/>
</signal>
<signal name="A5">
<contactref element="IC1" pad="T"/>
<contactref element="X4" pad="31"/>
</signal>
<signal name="A6">
<contactref element="IC1" pad="S"/>
<contactref element="X4" pad="29"/>
</signal>
<signal name="A7">
<contactref element="IC1" pad="R"/>
<contactref element="X4" pad="27"/>
</signal>
<signal name="A8">
<contactref element="IC1" pad="P"/>
<contactref element="X4" pad="25"/>
</signal>
<signal name="A9">
<contactref element="IC1" pad="N"/>
<contactref element="X4" pad="23"/>
</signal>
<signal name="A10">
<contactref element="IC1" pad="M"/>
<contactref element="X4" pad="21"/>
</signal>
<signal name="A11">
<contactref element="IC1" pad="L"/>
<contactref element="X4" pad="19"/>
</signal>
<signal name="A12">
<contactref element="IC1" pad="K"/>
<contactref element="X4" pad="17"/>
</signal>
<signal name="A13">
<contactref element="IC1" pad="J"/>
<contactref element="X4" pad="15"/>
</signal>
<signal name="A14">
<contactref element="IC1" pad="H"/>
<contactref element="X4" pad="13"/>
</signal>
<signal name="A15">
<contactref element="IC1" pad="F"/>
<contactref element="X4" pad="11"/>
</signal>
<signal name="!IRQ">
<contactref element="IC1" pad="4"/>
<contactref element="X4" pad="8"/>
</signal>
<signal name="BA">
<contactref element="IC1" pad="12"/>
<contactref element="X4" pad="24"/>
</signal>
<signal name="!ROML">
<contactref element="IC1" pad="11"/>
<contactref element="X4" pad="22"/>
</signal>
<signal name="!NMI">
<contactref element="IC1" pad="D"/>
<contactref element="X4" pad="7"/>
</signal>
<signal name="DOTCLK">
<contactref element="IC1" pad="6"/>
<contactref element="X4" pad="12"/>
</signal>
<signal name="!ROMH">
<contactref element="IC1" pad="B"/>
<contactref element="X4" pad="3"/>
</signal>
<signal name="R!W">
<contactref element="IC1" pad="5"/>
<contactref element="X4" pad="10"/>
</signal>
<signal name="!IO1">
<contactref element="IC1" pad="7"/>
<contactref element="X4" pad="14"/>
</signal>
<signal name="!IO2">
<contactref element="IC1" pad="10"/>
<contactref element="X4" pad="20"/>
</signal>
<signal name="!EXROM">
<contactref element="IC1" pad="9"/>
<contactref element="X4" pad="18"/>
</signal>
<signal name="!GAME">
<contactref element="IC1" pad="8"/>
<contactref element="X4" pad="16"/>
</signal>
<signal name="PHI2">
<contactref element="IC1" pad="E"/>
<contactref element="X4" pad="9"/>
</signal>
<signal name="!RES">
<contactref element="IC1" pad="C"/>
<contactref element="X4" pad="5"/>
<contactref element="S1" pad="1"/>
</signal>
<signal name="!DMA">
<contactref element="IC1" pad="13"/>
<contactref element="X4" pad="26"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
